OPTIGRÜN International AG
Optigrün International AG 
Am Birkenstock 15-19 
G 72505 Krauchenwies-Göggingen
Phone +49 (0)7576 772-0 
Fax +49 (0)7576 772-299 
info@optigruen.de 
technik@optigruen.de 
www.optigreen.com

....m² 	Optigreen Protection, Separation and Glide Fleece Type SGL 500 and 1 layer 	Optigreen HDPE Slip Sheet with a thickness of 0.2 mm as a slip 	layer

....m² 	Optigreen Drainage Board Type FKD 60 (BU) as a pressure-stable, vehicle 	drainage layer, filled with Perl 8-16

....m² 	Optigreen Filter Fleece Type 300 as filter layer

....m² 	>300 mm mineral gravel base 0-32 or 0-45 mm 

....m² 	30 - 50 mm Optigreen Substrat for Greenable Surfaces Type BB

....m²	grass grid pavers (100 - 140 mm)

....m² 	lawn seed type RMS 5.1 or 7.2 for heavily-used lawns